(kicad_symbol_lib (version 20210619) (generator kicad_symbol_editor)
  (symbol "Mereni_01:Ampermetr_horizontalni" (pin_numbers hide) (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -3.302 1.016 0))
    (property "Value" "Ampermetr_horizontalni" (id 1) (at -3.302 -0.762 0))
    (property "Footprint" "" (id 2) (at 0 2.54 90))
    (property "Datasheet" "~" (id 3) (at 0 2.54 90))
    (property "ki_keywords" "ammeter DC ampere meter" (id 4) (at 0 0 0))
    (property "ki_description" "DC ampermetr" (id 5) (at 0 0 0))
    (symbol "Ampermetr_horizontalni_0_0"
      (text "A" (at 0 0 0))
    )
    (symbol "Ampermetr_horizontalni_0_1")
    (symbol "Ampermetr_horizontalni_1_1"
      (pin passive line (at 0 -5.08 90) (length 2.54)
        (name "-")
        (number "1")
      )
      (pin passive line (at 0 5.08 270) (length 2.54)
        (name "+")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:Ampermetr_vertikalni" (pin_numbers hide) (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -3.302 1.016 0))
    (property "Value" "Ampermetr_vertikalni" (id 1) (at -3.302 -0.762 0))
    (property "Footprint" "" (id 2) (at 0 2.54 90))
    (property "Datasheet" "~" (id 3) (at 0 2.54 90))
    (property "ki_keywords" "ammeter DC ampere meter" (id 4) (at 0 0 0))
    (property "ki_description" "DC ampermetr" (id 5) (at 0 0 0))
    (symbol "Ampermetr_vertikalni_0_0"
      (text "A" (at 0 0 0))
    )
    (symbol "Ampermetr_vertikalni_0_1")
    (symbol "Ampermetr_vertikalni_1_1"
      (pin passive line (at 5.08 0 180) (length 2.54)
        (name "-")
        (number "1")
      )
      (pin passive line (at -5.08 0 0) (length 2.54)
        (name "+")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:CP_elektrolyt" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "C" (id 0) (at 0.254 1.778 0))
    (property "Value" "CP_elektrolyt" (id 1) (at 0.254 -2.032 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "~" (id 3) (at 0 0 0))
    (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
    (property "ki_description" "Polarized capacitor, small symbol" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
    (symbol "CP_elektrolyt_0_1")
    (symbol "CP_elektrolyt_1_1"
      (pin passive line (at 0 2.54 270) (length 1.8542)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -2.54 90) (length 1.8542)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:CTRIM" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "C" (id 0) (at 1.524 -2.032 0))
    (property "Value" "CTRIM" (id 1) (at 3.048 -3.556 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "~" (id 3) (at 0 0 0))
    (property "ki_keywords" "trimmer variable capacitor" (id 4) (at 0 0 0))
    (property "ki_description" "Trimmable capacitor, small symbol" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
    (symbol "CTRIM_0_1")
    (symbol "CTRIM_1_1"
      (pin passive line (at 0 2.54 270) (length 2.032)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -2.54 90) (length 2.032)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:C_kondenzator" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "C" (id 0) (at 0.254 1.778 0))
    (property "Value" "C_kondenzator" (id 1) (at 0.254 -2.032 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "~" (id 3) (at 0 0 0))
    (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
    (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
    (symbol "C_kondenzator_0_1")
    (symbol "C_kondenzator_1_1"
      (pin passive line (at 0 2.54 270) (length 2.032)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -2.54 90) (length 2.032)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:Dioda" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (id 0) (at -1.27 2.032 0))
    (property "Value" "Dioda" (id 1) (at -3.81 -2.032 0))
    (property "Footprint" "" (id 2) (at 0 0 90))
    (property "Datasheet" "~" (id 3) (at 0 0 90))
    (property "ki_keywords" "diode" (id 4) (at 0 0 0))
    (property "ki_description" "Diode, small symbol" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
    (symbol "Dioda_0_1")
    (symbol "Dioda_1_1"
      (pin passive line (at -2.54 0 0) (length 1.778)
        (name "K")
        (number "1")
      )
      (pin passive line (at 2.54 0 180) (length 1.778)
        (name "A")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:Dvojbran" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.937 7.874 0))
    (property "Value" "Dvojbran" (id 1) (at 5.1562 4.9022 0))
    (property "Footprint" "" (id 2) (at -1.1938 2.3622 0))
    (property "Datasheet" "" (id 3) (at -1.1938 2.3622 0))
    (symbol "Dvojbran_0_0"
      (text "+" (at 3.81 12.7 0))
      (text "-" (at 3.81 -2.54 0))
      (text "GND" (at -2.54 3.81 0))
      (text "GND" (at 12.7 3.81 0))
      (text "OUT" (at 12.7 8.89 0))
    )
    (symbol "Dvojbran_0_1")
    (symbol "Dvojbran_1_1"
      (text " " (at 4.5212 5.3086 0))
      (text "IN" (at -2.54 8.89 0))
      (pin input line (at -2.54 2.54 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -2.54 7.62 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 5.08 -2.54 90) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 5.08 12.7 270) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 12.7 2.54 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 12.7 7.62 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Dvojbran_1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.937 7.874 0))
    (property "Value" "Dvojbran_1" (id 1) (at 5.1562 4.9022 0))
    (property "Footprint" "" (id 2) (at -1.1938 2.3622 0))
    (property "Datasheet" "" (id 3) (at -1.1938 2.3622 0))
    (symbol "Dvojbran_1_0_0"
      (text "GND" (at -2.54 3.81 0))
      (text "GND" (at 12.7 3.81 0))
      (text "OUT" (at 12.7 8.89 0))
    )
    (symbol "Dvojbran_1_0_1")
    (symbol "Dvojbran_1_1_1"
      (text " " (at 4.5212 5.3086 0))
      (text "IN" (at -2.54 8.89 0))
      (pin input line (at -2.54 2.54 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -2.54 7.62 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 12.7 2.54 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 12.7 7.62 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Generator" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 6.985 10.795 0))
    (property "Value" "Generator" (id 1) (at 6.35 17.78 0))
    (property "Footprint" "" (id 2) (at 15.24 27.94 0))
    (property "Datasheet" "" (id 3) (at 15.24 27.94 0))
    (symbol "Generator_0_1")
    (symbol "Generator_1_1"
      (text "CH1" (at 17.78 27.94 0))
      (text "CH2" (at 17.78 21.59 0))
      (text "Counter" (at 17.78 12.7 0))
      (text "Generator" (at 7.62 24.765 0))
      (text "GND" (at 17.78 6.35 0))
      (pin input line (at 16.51 3.81 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 16.51 10.16 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 16.51 19.05 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 16.51 25.4 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:L" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "L" (id 0) (at 0 2.54 0))
    (property "Value" "L" (id 1) (at 0 -1.27 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "~" (id 3) (at 0 0 0))
    (property "ki_keywords" "simulation" (id 4) (at 0 0 0))
    (property "ki_description" "Inductor symbol for simulation only" (id 5) (at 0 0 0))
    (symbol "L_0_1")
    (symbol "L_1_1"
      (pin input line (at -6.35 0 0) (length 1.27)
        (name "1")
        (number "1")
      )
      (pin input line (at 6.35 0 180) (length 1.27)
        (name "2")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (id 0) (at 0 2.54 0))
    (property "Value" "LED" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "~" (id 3) (at 0 0 0))
    (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
    (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
    (symbol "LED_0_1")
    (symbol "LED_1_1"
      (pin passive line (at -3.81 0 0) (length 2.54)
        (name "K")
        (number "1")
      )
      (pin passive line (at 3.81 0 180) (length 2.54)
        (name "A")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:MP3" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 12.827 7.874 0))
    (property "Value" "MP3" (id 1) (at 12.7762 4.9022 0))
    (property "Footprint" "" (id 2) (at -1.1938 2.3622 0))
    (property "Datasheet" "" (id 3) (at -1.1938 2.3622 0))
    (symbol "MP3_0_1")
    (symbol "MP3_1_1"
      (text "Z" (at 4.5212 5.3086 0))
      (pin input line (at 5.08 12.7 270) (length 2.54)
        (name "+")
        (number "~")
      )
      (pin input line (at 5.08 -2.54 90) (length 2.54)
        (name "I")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:MP4" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 12.827 7.874 0))
    (property "Value" "MP4" (id 1) (at 12.7762 4.9022 0))
    (property "Footprint" "" (id 2) (at -1.1938 2.3622 0))
    (property "Datasheet" "" (id 3) (at -1.1938 2.3622 0))
    (symbol "MP4_0_1")
    (symbol "MP4_1_1"
      (text "Z" (at 4.5212 5.3086 0))
      (pin input line (at 5.08 12.7 270) (length 2.54)
        (name "+")
        (number "~")
      )
      (pin input line (at 5.08 -2.54 90) (length 2.54)
        (name "I")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:MP5" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 12.827 7.874 0))
    (property "Value" "MP5" (id 1) (at 12.7762 4.9022 0))
    (property "Footprint" "" (id 2) (at -1.1938 2.3622 0))
    (property "Datasheet" "" (id 3) (at -1.1938 2.3622 0))
    (symbol "MP5_0_0"
      (text "GND" (at 2.54 -2.54 0))
      (text "OUT" (at 2.54 13.97 0))
    )
    (symbol "MP5_0_1")
    (symbol "MP5_1_1"
      (text "FG" (at 4.5212 5.3086 0))
      (pin input line (at 5.08 -2.54 90) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 5.08 12.7 270) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:NPN" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "NPN" (id 0) (at 5.08 1.905 0))
    (property "Value" "NPN" (id 1) (at 5.08 0 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 5.08 -1.905 0))
    (property "Datasheet" "http://www.fairchildsemi.com/ds/BC/BC547.pdf" (id 3) (at 0 0 0))
    (property "ki_keywords" "NPN Transistor" (id 4) (at 0 0 0))
    (property "ki_description" "0.1A Ic, 65V Vce, Small Signal NPN Transistor, TO-92" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "TO?92*" (id 6) (at 0 0 0))
    (symbol "NPN_0_1")
    (symbol "NPN_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "C")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.08)
        (name "B")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "E")
        (number "3")
      )
    )
  )
  (symbol "Mereni_01:OTDR" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "." (id 0) (at 10.795 6.985 90))
    (property "Value" "OTDR" (id 1) (at 17.78 7.62 0))
    (property "Footprint" "" (id 2) (at 16.51 -1.27 90))
    (property "Datasheet" "" (id 3) (at 16.51 -1.27 90))
    (symbol "OTDR_0_0"
      (text "FC - APC" (at -5.08 7.62 0))
    )
    (symbol "OTDR_0_1")
    (symbol "OTDR_1_1"
      (text "OTDR" (at 12.065 7.62 0))
      (pin input line (at -2.54 6.35 0) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Osciloskop" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "." (id 0) (at 8.255 17.145 0))
    (property "Value" "Osciloskop" (id 1) (at 8.89 10.16 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "Osciloskop_0_1")
    (symbol "Osciloskop_1_1"
      (text "CH1" (at -2.54 26.67 0))
      (text "CH2" (at -2.54 19.685 0))
      (text "EXT TRIG" (at -3.81 12.7 0))
      (text "GND" (at -2.54 5.08 0))
      (text "OSC" (at 7.62 3.175 0))
      (pin input line (at -1.27 2.54 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 10.16 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 17.78 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 24.13 0) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Osciloskop_1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "." (id 0) (at 10.795 6.985 90))
    (property "Value" "Osciloskop_1" (id 1) (at 17.78 7.62 0))
    (property "Footprint" "" (id 2) (at 16.51 -1.27 90))
    (property "Datasheet" "" (id 3) (at 16.51 -1.27 90))
    (symbol "Osciloskop_1_0_1")
    (symbol "Osciloskop_1_1_1"
      (text "CH1" (at 2.54 16.51 0))
      (text "CH2" (at 11.43 16.51 0))
      (text "EXTTRIG" (at 27.94 16.51 0))
      (text "GND" (at 10.16 -2.54 0))
      (text "OSC" (at 24.765 6.35 0))
      (pin input line (at 5.08 16.51 270) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 13.97 -2.54 90) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 13.97 16.51 270) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 22.86 16.51 270) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Osciloskop_3" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "." (id 0) (at 8.255 17.145 0))
    (property "Value" "Osciloskop_3" (id 1) (at 8.89 10.16 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "Osciloskop_3_0_1")
    (symbol "Osciloskop_3_1_1"
      (text "CH1" (at -1.905 26.035 0))
      (text "CH2" (at -2.54 19.685 0))
      (text "GND" (at -2.54 5.08 0))
      (text "OSC" (at 7.62 3.175 0))
      (text "TRIG" (at -2.54 10.795 0))
      (pin input line (at -1.27 2.54 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 8.89 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 17.78 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 24.13 0) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Pojistka" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "Pojistka" (id 0) (at -1.27 2.032 0))
    (property "Value" "Pojistka" (id 1) (at -1.27 0 0))
    (property "Footprint" "" (id 2) (at -1.27 0 90))
    (property "Datasheet" "~" (id 3) (at -1.27 0 90))
    (property "ki_keywords" "resistor simulation" (id 4) (at 0 0 0))
    (property "ki_description" "Resistor symbol for simulation only" (id 5) (at 0 0 0))
    (symbol "Pojistka_0_1")
    (symbol "Pojistka_1_1"
      (pin passive line (at -7.62 0 0) (length 2.54)
        (name "~")
        (number "1")
      )
      (pin passive line (at 5.08 0 180) (length 2.54)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:Prevodnik" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "." (id 0) (at 8.255 17.145 0))
    (property "Value" "Prevodnik" (id 1) (at 8.89 10.16 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "Prevodnik_0_0"
      (text "+" (at 16.51 20.32 0))
      (text "-" (at 16.51 6.35 0))
    )
    (symbol "Prevodnik_0_1")
    (symbol "Prevodnik_1_1"
      (text "1" (at 2.54 24.13 0))
      (text "2" (at 2.54 17.78 0))
      (text "3" (at 2.54 10.16 0))
      (text "4" (at 2.54 2.54 0))
      (text "Prevodnik" (at 8.89 2.54 0))
      (pin input line (at -1.27 2.54 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 8.89 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 17.78 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 24.13 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 20.32 6.35 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 20.32 20.32 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:R_potenciometr" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "RV" (id 0) (at -4.445 0 90))
    (property "Value" "R_potenciometr" (id 1) (at -2.54 0 90))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "~" (id 3) (at 0 0 0))
    (property "ki_keywords" "resistor variable" (id 4) (at 0 0 0))
    (property "ki_description" "Potentiometer" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "Potentiometer*" (id 6) (at 0 0 0))
    (symbol "R_potenciometr_0_1")
    (symbol "R_potenciometr_1_1"
      (pin passive line (at 0 2.54 270) (length 0.635)
        (name "1")
        (number "1")
      )
      (pin passive line (at 2.54 0 180) (length 0.9906)
        (name "2")
        (number "2")
      )
      (pin passive line (at 0 -2.54 90) (length 0.635)
        (name "3")
        (number "3")
      )
    )
  )
  (symbol "Mereni_01:Rezistor" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (id 0) (at 2.032 0 90))
    (property "Value" "Rezistor" (id 1) (at 0 0 90))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "~" (id 3) (at 0 0 0))
    (property "ki_keywords" "resistor simulation" (id 4) (at 0 0 0))
    (property "ki_description" "Resistor symbol for simulation only" (id 5) (at 0 0 0))
    (symbol "Rezistor_0_1")
    (symbol "Rezistor_1_1"
      (pin passive line (at 0 6.35 270) (length 2.54)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -6.35 90) (length 2.54)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:Snimac" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.937 7.874 0))
    (property "Value" "Snimac" (id 1) (at 5.1562 4.9022 0))
    (property "Footprint" "" (id 2) (at -1.1938 2.3622 0))
    (property "Datasheet" "" (id 3) (at -1.1938 2.3622 0))
    (symbol "Snimac_0_0"
      (text "L+" (at 12.7 10.16 0))
      (text "M" (at 12.7 2.54 0))
      (text "Q" (at 12.7 6.35 0))
    )
    (symbol "Snimac_0_1")
    (symbol "Snimac_1_1"
      (text " " (at 4.5212 5.3086 0))
      (pin input line (at 12.7 1.27 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 12.7 5.08 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 12.7 8.89 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Snimac_1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 6.985 10.795 0))
    (property "Value" "Snimac_1" (id 1) (at 6.35 17.78 0))
    (property "Footprint" "" (id 2) (at 15.24 27.94 0))
    (property "Datasheet" "" (id 3) (at 15.24 27.94 0))
    (symbol "Snimac_1_0_1")
    (symbol "Snimac_1_1_1"
      (text "ALL IN " (at 6.985 2.54 0))
      (text "L+" (at 17.78 27.94 0))
      (text "M" (at 17.78 6.35 0))
      (text "Q" (at 17.78 21.59 0))
      (text "Qa" (at 17.78 12.7 0))
      (text "Snímač" (at 7.62 24.765 0))
      (pin input line (at 16.51 3.81 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 16.51 10.16 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 16.51 19.05 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 16.51 25.4 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Spektralni_analyzator" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 17.78 15.24 0))
    (property "Value" "Spektralni_analyzator" (id 1) (at 16.51 12.7 0))
    (property "Footprint" "" (id 2) (at -1.1938 2.3622 0))
    (property "Datasheet" "" (id 3) (at -1.1938 2.3622 0))
    (symbol "Spektralni_analyzator_0_0"
      (text "OPTO" (at 13.97 7.62 0))
      (text "USB" (at -3.81 7.62 0))
    )
    (symbol "Spektralni_analyzator_0_1")
    (symbol "Spektralni_analyzator_1_1"
      (text "SA" (at 4.5212 5.3086 0))
      (pin input line (at -2.54 5.08 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 12.7 5.08 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Symetricky_zdroj" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 17.78 15.24 0))
    (property "Value" "Symetricky_zdroj" (id 1) (at 16.51 12.7 0))
    (property "Footprint" "" (id 2) (at -1.1938 2.3622 0))
    (property "Datasheet" "" (id 3) (at -1.1938 2.3622 0))
    (symbol "Symetricky_zdroj_0_0"
      (text "+" (at 2.54 13.97 0))
      (text "-" (at 2.54 -2.54 0))
      (text "GND" (at 13.97 7.62 0))
    )
    (symbol "Symetricky_zdroj_0_1")
    (symbol "Symetricky_zdroj_1_1"
      (text "Z" (at 4.5212 5.3086 0))
      (pin input line (at 5.08 -2.54 90) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 5.08 12.7 270) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at 12.7 5.08 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:UNIMA" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 8.255 17.145 0))
    (property "Value" "UNIMA" (id 1) (at 8.89 10.16 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "UNIMA_0_1")
    (symbol "UNIMA_1_1"
      (text "ALL IN " (at 8.255 25.4 0))
      (text "Generátor" (at 7.62 3.175 0))
      (text "GND" (at -2.54 5.08 0))
      (text "GND" (at -2.54 19.685 0))
      (text "IN" (at -1.905 26.035 0))
      (text "OUT" (at -2.54 10.795 0))
      (pin input line (at -1.27 2.54 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 8.89 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 17.78 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 24.13 0) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:UNIMA_1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 8.255 17.145 0))
    (property "Value" "UNIMA_1" (id 1) (at 8.89 10.16 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "UNIMA_1_0_1")
    (symbol "UNIMA_1_1_1"
      (text "ALL IN " (at 8.255 25.4 0))
      (text "Generátor" (at 7.62 3.175 0))
      (text "GND" (at -2.54 19.685 0))
      (text "IN" (at -1.905 26.035 0))
      (pin input line (at -1.27 17.78 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 24.13 0) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:UNIMA_2" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 8.255 17.145 0))
    (property "Value" "UNIMA_2" (id 1) (at 8.89 10.16 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "UNIMA_2_0_0"
      (text "B" (at -2.54 20.32 0))
    )
    (symbol "UNIMA_2_0_1")
    (symbol "UNIMA_2_1_1"
      (text "A" (at -3.175 26.035 0))
      (text "ALL IN " (at 8.255 25.4 0))
      (text "Generátor" (at 7.62 3.175 0))
      (text "GND" (at -2.54 5.08 0))
      (text "GND" (at -2.54 15.875 0))
      (text "OUT" (at -2.54 9.525 0))
      (pin input line (at -1.27 2.54 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 7.62 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin output line (at -1.27 13.97 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 19.05 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -1.27 24.13 0) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Voltmetr_horizontalni" (pin_numbers hide) (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "V" (id 0) (at -3.302 1.016 0))
    (property "Value" "Voltmetr_horizontalni" (id 1) (at -3.302 -0.762 0))
    (property "Footprint" "" (id 2) (at 0 2.54 90))
    (property "Datasheet" "~" (id 3) (at 0 2.54 90))
    (property "ki_keywords" "ammeter DC ampere meter" (id 4) (at 0 0 0))
    (property "ki_description" "DC ampermetr" (id 5) (at 0 0 0))
    (symbol "Voltmetr_horizontalni_0_0"
      (text "V" (at 0 0 0))
    )
    (symbol "Voltmetr_horizontalni_0_1")
    (symbol "Voltmetr_horizontalni_1_1"
      (pin passive line (at 0 -5.08 90) (length 2.54)
        (name "-")
        (number "1")
      )
      (pin passive line (at 0 5.08 270) (length 2.54)
        (name "+")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:Voltmetr_vertikalni" (pin_numbers hide) (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "V" (id 0) (at -3.302 1.016 0))
    (property "Value" "Voltmetr_vertikalni" (id 1) (at -3.302 -0.762 0))
    (property "Footprint" "" (id 2) (at 0 2.54 90))
    (property "Datasheet" "~" (id 3) (at 0 2.54 90))
    (property "ki_keywords" "ammeter DC ampere meter" (id 4) (at 0 0 0))
    (property "ki_description" "DC ampermetr" (id 5) (at 0 0 0))
    (symbol "Voltmetr_vertikalni_0_0"
      (text "V" (at 0 0 0))
    )
    (symbol "Voltmetr_vertikalni_0_1")
    (symbol "Voltmetr_vertikalni_1_1"
      (pin passive line (at 5.08 0 180) (length 2.54)
        (name "-")
        (number "1")
      )
      (pin passive line (at -5.08 0 0) (length 2.54)
        (name "+")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:Wobbler" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -9.525 23.495 0))
    (property "Value" "Wobbler" (id 1) (at -14.605 -6.985 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "Wobbler_0_0"
      (text "ALL IN " (at -14.605 19.685 0))
      (text "Generátor" (at -15.24 -2.54 0))
      (text "GND" (at -25.4 -0.635 0))
      (text "GND" (at -25.4 15.24 0))
      (text "IN" (at -24.765 21.59 0))
      (text "OUT" (at -25.4 7.62 0))
      (text "Wobbler" (at -15.24 8.89 0))
    )
    (symbol "Wobbler_0_1")
    (symbol "Wobbler_1_1"
      (pin input line (at -24.765 -3.175 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -24.765 4.445 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -24.765 12.7 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -24.765 19.685 0) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Zarovka" (pin_numbers hide) (pin_names (offset 0.0254) hide) (in_bom yes) (on_board yes)
    (property "Reference" "Z" (id 0) (at -3.302 1.016 0))
    (property "Value" "Zarovka" (id 1) (at -3.302 -0.762 0))
    (property "Footprint" "" (id 2) (at 0 2.54 90))
    (property "Datasheet" "~" (id 3) (at 0 2.54 90))
    (property "ki_description" "žárovka" (id 4) (at 0 0 0))
    (symbol "Zarovka_0_0"
      (text " " (at 0 0 0))
    )
    (symbol "Zarovka_0_1")
    (symbol "Zarovka_1_1"
      (pin passive line (at 0 -5.08 90) (length 2.54)
        (name "-")
        (number "1")
      )
      (pin passive line (at 0 5.08 270) (length 2.54)
        (name "+")
        (number "2")
      )
    )
  )
  (symbol "Mereni_01:Zesilovac" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "Zesilovac" (id 0) (at -24.638 0.254 0))
    (property "Value" "Zesilovac" (id 1) (at -25.4 2.54 0))
    (property "Footprint" "" (id 2) (at -25.4 2.54 0))
    (property "Datasheet" "" (id 3) (at -25.4 2.54 0))
    (symbol "Zesilovac_0_1")
    (symbol "Zesilovac_1_1"
      (text "GND" (at -42.926 2.286 0))
      (text "GND" (at -8.382 2.032 0))
      (text "L IN" (at -43.942 -1.778 0))
      (text "L OUT" (at -7.366 -1.524 0))
      (text "R IN" (at -42.926 6.858 0))
      (text "R OUT" (at -7.62 7.112 0))
      (text "Vstup" (at -36.195 0.9906 0))
      (text "Výstup" (at -14.732 0.8636 0))
      (pin input line (at -41.91 -3.81 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -41.91 0 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -41.91 5.08 0) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -8.89 -3.81 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -8.89 0 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -8.89 5.08 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "Mereni_01:Zesilovac_1" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "Zesilovac" (id 0) (at -34.798 12.954 0))
    (property "Value" "Zesilovac_1" (id 1) (at -34.163 15.6464 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "Zesilovac_1_0_0"
      (text "GND" (at -25.4 7.62 0))
      (text "GND" (at -25.146 25.4 0))
      (text "L IN" (at -25.4 11.938 0))
      (text "L OUT" (at -24.384 29.718 0))
      (text "R IN" (at -25.146 3.81 0))
      (text "R OUT" (at -23.876 21.336 0))
    )
    (symbol "Zesilovac_1_0_1")
    (symbol "Zesilovac_1_1_1"
      (text "Vstup" (at -35.2044 6.35 0))
      (text "Výstup" (at -35.8394 24.765 0))
      (pin input line (at -25.4 2.54 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -25.4 6.35 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin input line (at -25.4 10.16 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin output line (at -25.4 20.32 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin output line (at -25.4 24.13 180) (length 2.54)
        (name "~")
        (number "~")
      )
      (pin output line (at -25.4 27.94 180) (length 2.54)
        (name "~")
        (number "~")
      )
    )
  )
)
